{"text_format":"3","workbook":"xls","n_sheets":5,"sheets":["c6zYcI","aF6TKw","BNdLQG","抽拔电缆","外委敷设电缆"],"not_rendered":{"external_links":1,"defined_names":1},"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"c6zYcI","index":0,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"aF6TKw","index":1,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"BNdLQG","index":2,"n_rows":0,"n_cols":0,"rows_kept":0,"hidden":true,"flags":["formulas_cached_only"]}

{"sheet":"抽拔电缆","index":3,"n_rows":74,"n_cols":9,"rows_kept":74,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["2023年度大修外委抽拔电缆一览表"]
["序号","装置","设备位号\n（项目名称）\n","用途","主控室位置\n（或电缆起始位置）","现场位置","电缆规格型号","预估电缆长度（米）","备注"]
[1,"合成氨","01TV-5060A","氨合成塔01R0501一床层温度调节","大主控中央控制室机柜间DP11-AOR09-6","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",500]
[2,"合成氨","01TV-5061A","氨合成塔01R0501二床层温度调节","大主控中央控制室机柜间DP81-AOR09-4","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",500]
[3,"合成氨","01LT-5021A","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间C2S2M01-6","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[4,"合成氨","01LT-5021B","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间C2S2M01-7","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[5,"合成氨","01LT-5021C ","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间C2S2M01-8","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[6,"合成氨","01LT-5020","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间DP81-AIR06-0","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[7,"合成氨","01HV-5010(反馈2根，电磁阀1根)","开工加热炉01B0501入口燃料气调节","大主控中央控制室机柜间C2S4M01-3","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",450]
[8,"合成氨","01HV-5011(反馈2根，电磁阀1根)","开工加热炉01B0501入口燃料气调节","大主控中央控制室机柜间C2S4M01-4","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",450]
[9,"合成氨","01HV-5012(反馈2根，电磁阀1根)","开工加热炉01B0501入口燃料气排放调节","大主控中央控制室机柜间C2S4M01-5","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",450]
[10,"合成氨","01HV-5031","中压蒸汽发生器01E0509排污调节","大主控中央控制室机柜间DP11-AOR09-3","一楼","1×2×1.5mm2本安电缆",500]
[11,"合成氨","01PV-5030 ","中压蒸汽发生器01E0509蒸汽压力调节 ","大主控中央控制室机柜间DP11-AOR09-5","一楼","1×2×1.5mm2本安电缆",500]
[12,"合成氨","01PT-5030","中压蒸汽发生器01E0509蒸汽压力 ","大主控中央控制室机柜间DP81-AIR06-1","一楼","1×2×1.5mm2本安电缆",500]
[13,"合成氨","01LV-5020","中压蒸汽发生器01E0509蒸汽液位调节 ","大主控中央控制室机柜间DP11-AOR09-4","一楼","1×2×1.5mm2本安电缆",500]
[14,"合成氨","01PT-5024","去氨罐冷氨压力","大主控中央控制室机柜间DP83-AI08","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[15,"合成氨","01FT-5031","1床调温线流量","大主控中央控制室机柜间DP21-AIR04-6","氨合成塔二楼平台上","1×2×1.5mm2本安电缆",500]
[16,"合成氨","01FT-5032","1#主线流量","大主控中央控制室机柜间DP21-AIR04-7","氨合成塔二楼平台上","1×2×1.5mm2本安电缆",500]
[17,"合成氨","01FT-5033","中压蒸汽发生器蒸汽流量","大主控中央控制室机柜间DP81-AIR05-6","一楼","1×2×1.5mm2本安电缆",500]
[18,"合成氨","01PDT-5031","氨合成塔01R0501出/入口合成器差压","大主控中央控制室机柜间DP21-AI12-7","一楼","1×2×1.5mm2本安电缆",500]
[19,"合成氨","01PT-5018A","开工加热炉01B0501入口燃料气压力","大主控中央控制室机柜间C2S2M01-2","01B0501入口燃料气压力，一楼","1×2×1.5mm2本安电缆",500]
[20,"合成氨","01PT-5018B","开工加热炉01B0501入口燃料气压力","大主控中央控制室机柜间C2S2MO1-2","01B0501入口燃料气压力，一楼","1×2×1.5mm2本安电缆",500]
[21,"合成氨","01FT-5004","开工加热炉01B0501入口燃料气","大主控中央控制室机柜间DP21-AI11-6","一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[22,"合成氨","01HV-5020","开工加热炉入口合成气","大主控中央控制室机柜间DP21-AOR07-3","一楼","1×2×1.5mm2本安电缆",500]
[23,"合成氨","01PDT-5025","氨合成塔出入口合成气压差","大主控中央控制室机柜间C2S1M05-3","一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[24,"合成氨","01PV-5018A","开工加热炉01B0501入口燃料气压力调节","大主控中央控制室机柜间DP21-AOR08-1","一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[25,"合成氨","01FT-5019（两根线）","去尿素装置热氨","大主控中央控制室机柜间DP21-AI11-6","一楼，热氨泵旁，两根线质量流量计","1×2×1.5mm2本安电缆",500]
[26,"合成氨","01LT-5010","氨冰机01S0502液位","大主控中央控制室机柜间C2S2-30044","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[27,"合成氨","01LT-5011","氨冰机01V505液位","大主控中央控制室机柜间C2S2-30043","氨冷冻框架顶楼","1×2×1.5mm2本安电缆",500]
[28,"合成氨","01TT-5004","开工加热炉出口合成气温度","大主控中央控制室机柜间DP21-AI11-10","带温变，01HV-5020上面管道上","1×2×1.5mm2本安电缆",500]
[29,"合成氨","01LT-5015A","氨合成汽包01V0502液位","大主控中央控制室机柜间DP83-AI07","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[30,"合成氨","           01LT-5015B","           氨合成汽包01V0502液位","大主控中央控制室机柜间 DP83-AI07","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[31,"合成氨","           01LT-5015C","           氨合成汽包01V0502液位","大主控中央控制室机柜间 DP83-AI07 ","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[32,"合成氨","            01LT-5012","           氨冰机01V504液位","   大主控中央控制室机柜间 C2S2-30046","         氨冷冻框架顶楼","1×2×1.5mm2本安电缆",500]
[33,"合成氨","           01FT-5003","           开工加热炉01B0501入口合成气","    大主控中央控制室机柜间DP21-AI11","        一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[34,"合成氨","           01LT-5009A","            氨分离器液位","    大主控中央控制室机柜间 C2S2M04-8/4","        氨分离器液位01S0501","1×2×1.5mm2本安电缆",400]
[35,"合成氨","           01LT-5009B","            氨分离器液位","    大主控中央控制室机柜间 C2S2M04-8/4 ","        氨分离器液位01S0501","1×2×1.5mm2本安电缆",400]
[36,"合成氨","         01PT-5003","            开工加热炉01B0501压力","    大主控中央控制室机柜间DP21-AI12","             一楼","1×2×1.5mm2本安电缆",500]
[37,"合成氨","         01PT-5019","            开工加热炉燃烧气压力","    大主控中央控制室机柜间DP21-AI12","         开工加热炉二楼平台","1×2×1.5mm2本安电缆",500]
[38,"合成氨","         01PT-5004","            氨合成塔01R0501出口压力","    大主控中央控制室机柜间DP21-AI12","        氨合成塔二楼平台上","1×2×1.5mm2本安电缆",500]
[39,"合成氨","         01FT-5007","            来自合成气压缩机合成气流量","   大主控中央控制室机柜间DP83-AI08","         一楼，热氨泵旁","1×2×1.5mm2本安电缆",500]
[40,"合成氨","         01FT-5018","            去罐区冷氨流量","大主控中央控制室机柜间DP83-AI09","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[41,"合成氨","         01PT-5006 ","           来自合成气压缩机合成气压力","大主控中央控制室机柜间DP83-AI08","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[42,"合成氨","        01PT-5007","            去合成气压缩机合成气压力"," 大主控中央控制室机柜间DP83-AI08","一楼,01LV-5005旁边","1×2×1.5mm2本安电缆",500]
[43,"合成氨","        01TV-5016","          合成蒸汽过热器01E0502出口温度调节"," 大主控中央控制室机柜间DP21-AOR08-5","一楼，合成蒸汽过热器01E0502出口温度)","1×2×1.5mm2本安电缆",500]
[44,"合成氨","        01FT-5020","          氨合成汽包01V0502入口锅炉给水流量"," 大主控中央控制室机柜间DP21-AI06-5","氨合成汽包旁","1×2×1.5mm2本安电缆",500]
[45,"合成氨","         01TT-5016","          合成蒸汽过热器01E0502出口温度"," 大主控中央控制室机柜间DP21-AIR05-4","一楼","1×2×1.5mm2本安电缆",500]
[46,"合成氨","01FV-5020/01LV-5001 ","氨合成回路汽包锅炉给水流量调节/氨合成汽包01V0502液位调节"," 大主控中央控制室机柜间DP21-AO07/DP21-AOR09-6","氨合成塔汽包旁，01V0502入口","1×2×1.5mm2本安电缆",500]
[47,"合成氨","01LT-5001","氨合成汽包01V0502液位 "," 大主控中央控制室机柜间DP21-AI04-6","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[48,"合成氨","01HV-5015","01S0502回流液"," 大主控中央控制室机柜间DP81-AOR09","一楼，冷氨泵旁","1×2×1.5mm2本安电缆",500]
[49,"合成氨","01TE-5021","去氨合成塔合成气温度"," 大主控中央控制室机柜间DP21-AI05-2","一楼，01TE-5019旁边","1×2×1.5mm2本安电缆",500]
[50,"合成氨","01TE-5041","冷氨泵出口氨温度"," 大主控中央控制室机柜间DP21-AI05-5","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[51,"合成氨","01TV-5021","去氨合成塔合成气温度调节"," 大主控中央控制室机柜间DP21-AOR08-6","一楼","1×2×1.5mm2本安电缆",500]
[52,"合成氨","01TE-5026","来自合成气压缩机合成气温度","大主控中央控制室机柜间DP23-RTD12-10 ","01FT-5018顶部红色管道上","1×3×1.5mm2本安电缆",500]
[53,"合成氨","01TE-5006","氨合成塔01R0501出口温度","大主控中央控制室机柜间DP23-RTD11-10 ","氨合成塔底部管线上","1×3×1.5mm2本安电缆",500]
[54,"合成氨","01TE-5015","合成蒸汽过热器01E0502出口温度"," 大主控中央控制室机柜间DP23-RTD11-10","一楼","1×3×1.5mm2本安电缆",500]
[55,"合成氨","01TE-5017","合成蒸汽过热器01E0502出口温度 "," 大主控中央控制室机柜间DP23-RTD12-10","一楼，合成气管道上","1×3×1.5mm2本安电缆",500]
[56,"合成氨","01TE-5049","二级闪蒸槽0V0505温度 "," 大主控中央控制室机柜间DP23-RTD12-10","氨冷冻框架顶楼","1×3×1.5mm2本安电缆",500]
[57,"合成氨","01TE-5050","一级闪蒸槽0V0504温度"," 大主控中央控制室机柜间DP23-RTD12-10","氨冷冻框架顶楼","1×3×1.5mm2本安电缆",500]
[58,"合成氨","01TJB-0505C","氨合成塔表面热电偶到大主控中央控制室机柜间"," 大主控中央控制室机柜间DP23","氨合成塔框架二楼平台中间接线箱","12×2×1.0mm2 K型补偿导线",450]
[59,"合成氨","01TJB-0506C ","氨合成塔表面热电偶到大主控中央控制室机柜间"," 大主控中央控制室机柜间DP23","氨合成塔框架二楼平台中间接线箱","12×2×1.0mm2 K型补偿导线",450]
[60,"合成氨","01TE-5060/61/62A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[61,"合成氨","01TE-5060/61/62A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[62,"合成氨","01TE-5063/64/65A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[63,"合成氨","01TE-5063/64/65A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[64,"合成氨","01TE-5052","开工加热炉01B0501温度 "," 大主控中央控制室机柜间DP23-TC09-10","开工加热炉二楼平台","1×2×1.5mm2  K型补偿导线",500]
[65,"合成氨","01TE-5053","开工加热炉01B0501温度"," 大主控中央控制室机柜间DP23-TC09-10","开工加热炉二楼平台","1×2×1.5mm2  K型补偿导线",500]
[66,"合成氨","01TE-5071A/B/C","氨合成塔01R0501壳体顶部表面温度"," 大主控中央控制室机柜间DP23 "," 氨合成塔底部","1×2×1.5mm2  K型补偿导线",150]
[67,"合成氨","01XT-5001A ","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[68,"合成氨","01XT-5001B ","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[69,"合成氨","01XT-5001C","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[70,"合成氨","01XT-5001D","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[71,"合成氨","01XT-5001E","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[72,"合成氨","01XT-5001F","开工加热炉火检"," 大主控中央控制室机柜间CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]

{"sheet":"外委敷设电缆","index":4,"n_rows":94,"n_cols":9,"rows_kept":94,"merged":[[0,0,0,8]],"flags":["formulas_cached_only"]}
["2023年度大修外委敷设电缆一览表"]
["序号","装置","设备位号\n（项目名称）\n","用途","主控室位置\n（或电缆起始位置）","现场位置","电缆规格型号","预估电缆长度（米）","备注"]
[1,"甲醇","03LT-7002","粗甲醇罐01V0701新增液位计","大主控中央控制室机柜间","甲醇中间罐区粗甲醇罐01V0701","ZR-DJYVPR-1×2×1.5mm2",500]
[2,"甲醇","01FT—40071A",null,"大主控中央控制室机柜间",null,"ZR-DJYVPR-1×2×1.5mm2",500]
[4,"甲醇","03XOV-5090","03S0503排放气动切断阀","大主控机柜间DCS系统","03S0503旁","ZR-DJYVPR 1×2×1.5mm 2 ",500]
[5,"甲醇","03XSO-5090","03S0503排放气动切断阀","大主控机柜间DCS系统","03S0503旁","ZR-DJYVPR 1×2×1.5mm 2 ",500]
[6,"甲醇","03XSC-5090","03S0503排放气动切断阀","大主控机柜间DCS系统","03S0503旁","ZR-DJYVPR 1×2×1.5mm 2 ",500]
[7,"合成氨","XSOV-5099A","液氨外排管线切断阀","大主控机柜间DCS系统","01LV-5002A/B旁","ZR-DJYVPR 1×2×1.5mm 2 ",450]
[8,"合成氨","XZSO-5099A","液氨外排管线切断阀","大主控机柜间DCS系统","01LV-5002A/B旁","ZR-DJYVPR 1×2×1.5mm 2 ",450]
[9,"合成氨","XZSC-5099A ","液氨外排管线切断阀","大主控机柜间DCS系统","01LV-5002A/B旁","ZR-DJYVPR 1×2×1.5mm 2 ",450]
[10,"合成氨","XSOV-5099B ","液氨外排管线切断阀","大主控机柜间DCS系统","01LV-5002A/B旁","ZR-DJYVPR 1×2×1.5mm 2 ",450]
[11,"合成氨","XZSO-5099B  ","液氨外排管线切断阀","大主控机柜间DCS系统","01LV-5002A/B旁","ZR-DJYVPR 1×2×1.5mm 2 ",450]
[12,"合成氨","XZSC-5099B","液氨外排管线切断阀","大主控机柜间DCS系统","01LV-5002A/B旁","ZR-DJYVPR 1×2×1.5mm 2 ",450]
[13,"合成氨","01TV-5060A","氨合成塔01R0501一床层温度调节","大主控中央控制室机柜间DP11-AOR09-6","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",500]
[14,"合成氨","01TV-5061A","氨合成塔01R0501二床层温度调节","大主控中央控制室机柜间DP81-AOR09-4","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",500]
[15,"合成氨","01LT-5021A","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间C2S2M01-6","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[16,"合成氨","01LT-5021B","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间C2S2M01-7","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[17,"合成氨","01LT-5021C ","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间C2S2M01-8","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[18,"合成氨","01LT-5020","中压蒸汽发生器01E0509蒸汽液位","大主控中央控制室机柜间DP81-AIR06-0","一楼，01E0509旁","1×2×1.5mm2本安电缆",500]
[19,"合成氨","01HV-5010(反馈2根，电磁阀1根)","开工加热炉01B0501入口燃料气调节","大主控中央控制室机柜间C2S4M01-3","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",450]
[20,"合成氨","01HV-5011(反馈2根，电磁阀1根)","开工加热炉01B0501入口燃料气调节","大主控中央控制室机柜间C2S4M01-4","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",450]
[21,"合成氨","01HV-5012(反馈2根，电磁阀1根)","开工加热炉01B0501入口燃料气排放调节","大主控中央控制室机柜间C2S4M01-5","一楼，氨合成塔底部","1×2×1.5mm2本安电缆",450]
[22,"合成氨","01HV-5031","中压蒸汽发生器01E0509排污调节","大主控中央控制室机柜间DP11-AOR09-3","一楼","1×2×1.5mm2本安电缆",500]
[23,"合成氨","01PV-5030 ","中压蒸汽发生器01E0509蒸汽压力调节 ","大主控中央控制室机柜间DP11-AOR09-5","一楼","1×2×1.5mm2本安电缆",500]
[24,"合成氨","01PT-5030","中压蒸汽发生器01E0509蒸汽压力 ","大主控中央控制室机柜间DP81-AIR06-1","一楼","1×2×1.5mm2本安电缆",500]
[25,"合成氨","01LV-5020","中压蒸汽发生器01E0509蒸汽液位调节 ","大主控中央控制室机柜间DP11-AOR09-4","一楼","1×2×1.5mm2本安电缆",500]
[26,"合成氨","01PT-5024","去氨罐冷氨压力","大主控中央控制室机柜间DP83-AI08","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[27,"合成氨","01FT-5031","1床调温线流量","大主控中央控制室机柜间DP21-AIR04-6","氨合成塔二楼平台上","1×2×1.5mm2本安电缆",500]
[28,"合成氨","01FT-5032","1#主线流量","大主控中央控制室机柜间DP21-AIR04-7","氨合成塔二楼平台上","1×2×1.5mm2本安电缆",500]
[29,"合成氨","01FT-5033","中压蒸汽发生器蒸汽流量","大主控中央控制室机柜间DP81-AIR05-6","一楼","1×2×1.5mm2本安电缆",500]
[30,"合成氨","01PDT-5031","氨合成塔01R0501出/入口合成器差压","大主控中央控制室机柜间DP21-AI12-7","一楼","1×2×1.5mm2本安电缆",500]
[31,"合成氨","01PT-5018A","开工加热炉01B0501入口燃料气压力","大主控中央控制室机柜间C2S2M01-2","01B0501入口燃料气压力，一楼","1×2×1.5mm2本安电缆",500]
[32,"合成氨","01PT-5018B","开工加热炉01B0501入口燃料气压力","大主控中央控制室机柜间C2S2MO1-2","01B0501入口燃料气压力，一楼","1×2×1.5mm2本安电缆",500]
[33,"合成氨","01FT-5004","开工加热炉01B0501入口燃料气","大主控中央控制室机柜间DP21-AI11-6","一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[34,"合成氨","01HV-5020","开工加热炉入口合成气","大主控中央控制室机柜间DP21-AOR07-3","一楼","1×2×1.5mm2本安电缆",500]
[35,"合成氨","01PDT-5025","氨合成塔出入口合成气压差","大主控中央控制室机柜间C2S1M05-3","一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[36,"合成氨","01PV-5018A","开工加热炉01B0501入口燃料气压力调节","大主控中央控制室机柜间DP21-AOR08-1","一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[37,"合成氨","01FT-5019（两根线）","去尿素装置热氨","大主控中央控制室机柜间DP21-AI11-6","一楼，热氨泵旁，两根线质量流量计","1×2×1.5mm2本安电缆",500]
[38,"合成氨","01LT-5010","氨冰机01S0502液位","大主控中央控制室机柜间C2S2-30044","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[39,"合成氨","01LT-5011","氨冰机01V505液位","大主控中央控制室机柜间C2S2-30043","氨冷冻框架顶楼","1×2×1.5mm2本安电缆",500]
[40,"合成氨","01TT-5004","开工加热炉出口合成气温度","大主控中央控制室机柜间DP21-AI11-10","带温变，01HV-5020上面管道上","1×2×1.5mm2本安电缆",500]
[41,"合成氨","01LT-5015A","氨合成汽包01V0502液位","大主控中央控制室机柜间DP83-AI07","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[42,"合成氨","           01LT-5015B","           氨合成汽包01V0502液位","    大主控中央控制室机柜间 DP83-AI07","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[43,"合成氨","           01LT-5015C","           氨合成汽包01V0502液位","    大主控中央控制室机柜间 DP83-AI07 ","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[44,"合成氨","            01LT-5012","           氨冰机01V504液位","   大主控中央控制室机柜间 C2S2-30046","         氨冷冻框架顶楼","1×2×1.5mm2本安电缆",500]
[45,"合成氨","           01FT-5003","           开工加热炉01B0501入口合成气","    大主控中央控制室机柜间DP21-AI11","        一楼，开工加热炉旁","1×2×1.5mm2本安电缆",500]
[46,"合成氨","           01LT-5009A","            氨分离器液位","    大主控中央控制室机柜间 C2S2M04-8/4","        氨分离器液位01S0501","1×2×1.5mm2本安电缆",400]
[47,"合成氨","           01LT-5009B","            氨分离器液位","    大主控中央控制室机柜间 C2S2M04-8/4 ","        氨分离器液位01S0501","1×2×1.5mm2本安电缆",400]
[48,"合成氨","         01PT-5003","            开工加热炉01B0501压力","    大主控中央控制室机柜间DP21-AI12","             一楼","1×2×1.5mm2本安电缆",500]
[49,"合成氨","         01PT-5019","            开工加热炉燃烧气压力","    大主控中央控制室机柜间DP21-AI12","         开工加热炉二楼平台","1×2×1.5mm2本安电缆",500]
[50,"合成氨","         01PT-5004","            氨合成塔01R0501出口压力","    大主控中央控制室机柜间DP21-AI12","        氨合成塔二楼平台上","1×2×1.5mm2本安电缆",500]
[51,"合成氨","         01FT-5007","            来自合成气压缩机合成气流量","   大主控中央控制室机柜间DP83-AI08","         一楼，热氨泵旁","1×2×1.5mm2本安电缆",500]
[52,"合成氨","         01FT-5018","            去罐区冷氨流量","大主控中央控制室机柜间DP83-AI09","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[53,"合成氨","         01PT-5006 ","           来自合成气压缩机合成气压力","大主控中央控制室机柜间DP83-AI08","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[54,"合成氨","        01PT-5007","            去合成气压缩机合成气压力"," 大主控中央控制室机柜间DP83-AI08","一楼,01LV-5005旁边","1×2×1.5mm2本安电缆",500]
[55,"合成氨","        01TV-5016","          合成蒸汽过热器01E0502出口温度调节"," 大主控中央控制室机柜间DP21-AOR08-5","一楼，合成蒸汽过热器01E0502出口温度)","1×2×1.5mm2本安电缆",500]
[56,"合成氨","        01FT-5020","          氨合成汽包01V0502入口锅炉给水流量"," 大主控中央控制室机柜间DP21-AI06-5","氨合成汽包旁","1×2×1.5mm2本安电缆",500]
[57,"合成氨","         01TT-5016","          合成蒸汽过热器01E0502出口温度"," 大主控中央控制室机柜间DP21-AIR05-4","一楼","1×2×1.5mm2本安电缆",500]
[58,"合成氨","01FV-5020/01LV-5001 ","氨合成回路汽包锅炉给水流量调节/氨合成汽包01V0502液位调节"," 大主控中央控制室机柜间DP21-AO07/DP21-AOR09-6","氨合成塔汽包旁，01V0502入口","1×2×1.5mm2本安电缆",500]
[59,"合成氨","01LT-5001","氨合成汽包01V0502液位 "," 大主控中央控制室机柜间DP21-AI04-6","合成氨汽包上","1×2×1.5mm2本安电缆",500]
[60,"合成氨","01HV-5015","01S0502回流液"," 大主控中央控制室机柜间DP81-AOR09","一楼，冷氨泵旁","1×2×1.5mm2本安电缆",500]
[61,"合成氨","01TE-5021","去氨合成塔合成气温度"," 大主控中央控制室机柜间DP21-AI05-2","一楼，01TE-5019旁边","1×2×1.5mm2本安电缆",500]
[62,"合成氨","01TE-5041","冷氨泵出口氨温度"," 大主控中央控制室机柜间DP21-AI05-5","一楼，联压厂房门口","1×2×1.5mm2本安电缆",500]
[63,"合成氨","01TV-5021","去氨合成塔合成气温度调节"," 大主控中央控制室机柜间DP21-AOR08-6","一楼","1×2×1.5mm2本安电缆",500]
[64,"合成氨","01TE-5026","来自合成气压缩机合成气温度","大主控中央控制室机柜间DP23-RTD12-10 ","01FT-5018顶部红色管道上","1×3×1.5mm2本安电缆",500]
[65,"合成氨","01TE-5006","氨合成塔01R0501出口温度","大主控中央控制室机柜间DP23-RTD11-10 ","氨合成塔底部管线上","1×3×1.5mm2本安电缆",500]
[66,"合成氨","01TE-5015","合成蒸汽过热器01E0502出口温度"," 大主控中央控制室机柜间DP23-RTD11-10","一楼","1×3×1.5mm2本安电缆",500]
[67,"合成氨","01TE-5017","合成蒸汽过热器01E0502出口温度 "," 大主控中央控制室机柜间DP23-RTD12-10","一楼，合成气管道上","1×3×1.5mm2本安电缆",500]
[68,"合成氨","01TE-5049","二级闪蒸槽0V0505温度 "," 大主控中央控制室机柜间DP23-RTD12-10","氨冷冻框架顶楼","1×3×1.5mm2本安电缆",500]
[69,"合成氨","01TE-5050","一级闪蒸槽0V0504温度"," 大主控中央控制室机柜间DP23-RTD12-10","氨冷冻框架顶楼","1×3×1.5mm2本安电缆",500]
[70,"合成氨","01TJB-0505C","氨合成塔表面热电偶到大主控中央控制室机柜间"," 大主控中央控制室机柜间DP23","氨合成塔框架二楼平台中间接线箱","12×2×1.0mm2 K型补偿导线",450]
[71,"合成氨","01TJB-0506C ","氨合成塔表面热电偶到大主控中央控制室机柜间"," 大主控中央控制室机柜间DP23","氨合成塔框架二楼平台中间接线箱","12×2×1.0mm2 K型补偿导线",450]
[72,"合成氨","01TE-5060/61/62A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[73,"合成氨","01TE-5060/61/62A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[74,"合成氨","01TE-5063/64/65A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[75,"合成氨","01TE-5063/64/65A-E ","氨合成塔床层多点热电偶到大主控中央控制室机柜间 "," 大主控中央控制室机柜间DP33","氨合成塔塔顶 ","12×2×1.0mm2 K型补偿导线",500]
[76,"合成氨","01TE-5052","开工加热炉01B0501温度 "," 大主控中央控制室机柜间DP23-TC09-10","开工加热炉二楼平台","1×2×1.5mm2  K型补偿导线",500]
[77,"合成氨","01TE-5053","开工加热炉01B0501温度"," 大主控中央控制室机柜间DP23-TC09-10","开工加热炉二楼平台","1×2×1.5mm2  K型补偿导线",500]
[78,"合成氨","01TE-5071A/B/C","氨合成塔01R0501壳体顶部表面温度"," 大主控中央控制室机柜间DP23 "," 氨合成塔底部","1×2×1.5mm2  K型补偿导线",150]
[79,"合成氨","01XT-5001A ","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[80,"合成氨","01XT-5001B ","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[81,"合成氨","01XT-5001C","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[82,"合成氨","01XT-5001D","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[83,"合成氨","01XT-5001E","开工加热炉火检"," 大主控中央控制室机柜间 CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[84,"合成氨","01XT-5001F","开工加热炉火检"," 大主控中央控制室机柜间CCR-ESD-002F-FTB14(C2S3M1)","开工加热炉底部","1×2×2.5mm2 火焰检测器专用本安电缆",500]
[85,"气化","01P0104E","气化新增低压料浆泵E信号及控制电缆预铺设","备煤厂房至气化机柜间","低压料浆泵A/B中间","ZR-DJYVPR-12×2×1.5mm2",300]
[86,"锅炉","08LV0801","08LV0801电缆敷设","锅炉主控","锅炉0米疏水泵处","ZC-DJYVRP-0.5kV\\2 x 2 x 1.5mm2",300]
[87,"锅炉","FT-SOHSG15 CF101","FT-SOHSG15 CF101流量计安装","脱硫主控","氨水制备","ZR-KVVP 1×2×1.5mm2 线芯为单股铜线\\24VDC",200]
[88,"锅炉","FT-1503","FT-1503流量计安装","脱硫主控","氨水制备","ZR-KVVP 1×2×1.5mm2 线芯为单股铜线\\24VDC",200]
[89,"锅炉","FT-32002","FT-32002流量计安装","脱硫主控","氨水制备","ZR-KVVP 1×2×1.5mm2 线芯为单股铜线\\24VDC",200]
[90,"锅炉","FT-0202","FT-0202流量计安装","脱硫主控","二期泵房","ZR-KVVP 1×2×1.5mm2 线芯为单股铜线\\24VDC",200]
[91,"锅炉","FV-1601","FV-1601阀门安装","脱硫主控","氨水制备","ZR-KVVP 1×2×1.5mm2 线芯为单股铜线\\24VDC",200]
[92,"空分",null,"空分新增气体检测器","空分主控室","空压机厂房","1×3×1.5mm2本安电缆",4500]
[93,"空分",null,"空分新增气体区域报警器","空分主控室","螺杆冰机机厂房","1×2×1.5mm2本安电缆",500]